Adamson's PLM Series preset for Adamson's Metrix Sub speaker.

Application Notes:
     CARDIOID MODE FBF : Front Back Front
     The preset is low-passed at 110 Hz 
     2 cabinets FRONT - 1 cabinet BACK

Routing:
     FRONT : 1
     BACK (front screen connector) : 2

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     V1.0

Designed by DV2
Pascal GUILLAUME