XE = quad amped


Each speaker is powered by a four channel PLM amplifier from Lab.gruppen.

Different from its sister monitor M3VE, a set of M3XE's is powered by not one, 
but two 12k44 Lab.gruppen amplifiers, 
using the integrated Lake active cross-over processing as well as powering the HF, 
MF and dual LF woofers by the four independent amplifier channels of the 12k44.

With the newest and most pristine Dynaudio ESOTAR driver technology, 
M3XE takes over where most other monitor systems give up. 
With unsurpassed attention to detail, underpinned by an impressive 22Hz - 21kHz 
frequency response and beyond 135dB SPL, 
M3XE leaves no room for desire in terms of resolution, range or sheer power.

