Outline's PLM Series presets suitable for Outline's Low pack CDL1815 speaker

Application notes:
2aux module for LOW pack CDL1815.

Amp.Gain 35 dB

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +5 dBu (LOWPACK 18"),+2dbu (LOWPACK 15") 
* ISVPL threshold at 153.0 Vpk (LOWPACK18"), 109.0 Vpk (LOWPACK 15")  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at
    +11 dBu-pk (LOWPACK 18"),+8 dbu-pk (LOWPACK 15")