Lab.gruppen's PLM Series preset suitable for L-Acoustics' ARCS speaker.

Application notes:
Created for the "ARCS 3W SB18 LO" application; 
ARCS + SB118 closely coupled (100 Hz crossover), 1:1 ratio, normal HF eq.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +9 dBu (SUB), +8 dBu (LF), +2 dBu (HF)
* ISVPL threshold at 160 Vpk (SUB), 130 Vpk (LF), 70 Vpk (HF)  

* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk