HK Audio VORTIS 2 preset suitable for Lab.Gruppen PLM 12k44 series. 


VORTIS 2 11510 90x55 - FR preset version:
* V1.0


Application notes:
* Designed to be used with VORTIS 2 11510 90x55
* Fullrange preset

 

Technical info:
* Amp Gain in module is set to 32dB. It can be switched down to 26dB in 0.1dB steps.
* MaxRMS limiter is active
* MaxPeak limiter threshold is +9dB, ISVPL is active

* Attention: For use with LM-series, please set MaxPeak limiter to 0dB


Support information:
* Internet: http://www.hkaudio.com
* E-Mail:   support(at)hkaudio.com
* Phone:    +49 (0) 6851 905-555
