Outline's PLM Series presets suitable for Outline's High Pack CDH483 speaker

Application notes:
2-way module for High Pack CDH483.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +3 dBu (MF), -2 dBu (HF)
* ISVPL threshold at 123.0 Vpk (MF), 69.2 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
     +9 dBu-pk (MF), +4 dBu-pk (HF)