Lab.gruppen's PLM Series preset suitable for JBL's VT4888 speaker.

Application notes:
Designed to be used together with "VT4880 for VT4888 60" preset.

The preset is a 3-way configuration, high-passed at 60 Hz.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +11 dBu (LF), +8.5 dBu (MF), +3.5 dBu (HF)
* ISVPL threshold at 154.8 Vpk (LF), 116.0 Vpk (MF), 65.0 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +14 dBu-pk (LF), +11.5 dBu-pk (MF), +6.5 dBu-pk (HF)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk
* To emulate 26 dB Amp Gain - set input gain to -6 dB

Fingerprint info:
VT4888 v1.0b1