Lab.gruppen's PLM Series preset suitable for L-Acoustics' dV-DOSC speaker.

Application notes:
Created for the "dV 3W 80 dV-SUB HI" application;  
Flown dV-DOSC + Ground Stacked dV-SUB (80 Hz crossover), 3:1 ratio, increased HF shelving eq.

NOTE! Can also be combined with other subwoofers using their 80 Hz preset, 
      but gain and delay may then have to be optimized. 

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (SUB), +6 dBu (LF), +1 dBu (HF)
* ISVPL threshold at 137.8 Vpk (SUB), 109.6 Vpk (LF), 61.6 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (SUB), +11 dBu-pk (LF), +6 dBu-pk (HF)

Fingerprint info:
dV-DOSC + dV-SUB v1.0 beta1