*** TURBOSOUND MANCHESTER Series ***
***       V1.0 RELEASE           ***
____________________________________________________

Air loss affects the HF performance of every loudspeaker system. 

This set of AirEQ filters will ensure a balanced high frequency response, 
and will discourage excessive boosting of frequencies that have no chance 
of reaching a listener compromising the HF dynamic performance of your system.
It is optimised for a distance of 15 meters.

Notes:
 
1) do not insert more than one filter at the same time.

2) other sets of filter is available for higher distances.

For intermediate distance use the closer available.

Please read the MANCHESTER series QSG and Rigging Manual prior to use 

*** Designed by Music Tribe - 05 DEC 2019 ***
http://www.turbosound.com
https://www.turbosound.com/brand/turbosound/support#googtrans(en|en)