Lab.gruppen's PLM Series preset suitable for L-Acoustics' SB18 speaker.

Application notes:
The preset is low-passed at 60 Hz, for use in combination with e.g. 
KAKA or k-systems.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10 dBu (SUB)
* ISVPL threshold at 160 Vpk (SUB)
* Input delay is set to align with system amP  

* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk