Lab.guppen's PLM Series preset suitable for NEXO's S1210 speaker.

Application Notes:
Preset created for a "S1210 wideband passive NXS" application. 

It is a 1+1 module so that it can be loaded together with a 
1+1 subwoofer file in the same PLM for a 2-way stereo setup.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at 475 W per cabinet (FR)
* ISVPL threshold at 144 Vpk (FR, primarily to avoid clipping the PLM)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)