Lake preset for ADAMSON E119
========================

Application Notes:
     - Front-Back-Front cardioid configuration
     - No linear phase compensation delay included (add 5 ms for linear phase compensation)
     - Low passed at 80 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - Front: Ch. 1 
     - Module out 2 -  Back: Ch. 2 (Use front connector) 

Technical Info:
     - Fingerprint: V1.0

=======================
Designed by ADAMSON & DV2