Tannoy's PLM Series preset suitable for Tannoy's VQ40/VS15DR speakers.

Application notes:
The preset is a 3-way configuration, with fixed crossover at 470 Hz 
between the LF section (VS15DR) and the Mid-High (VQ40). 
The LF section is high-passed at 40 Hz (12dB/oct Butterworth).

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10.0 dBu (SUB), +2.0 dBu (MF), -1.0 dBu (HF)
* ISVPL threshold at n/a (SUB), 97.6 Vpk (MF), 69.0 Vpk (HF)