Lab.gruppen's PLM Series preset suitable for L-Acoustics' SB118 speaker.

Application notes:
1+1 module created for the "SB118 80 Hz" application.
If used together with KUDO; then use "KUDO 80 Hz LO/HI". Each of the 
2 identical subwoofer channels has a separate input mixer to allow for 
a Left and Right subwoofer that only uses one module.  

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10 dBu (SUB)
* ISVPL threshold at 173.7 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +15 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk