Lake preset for ADAMSON S119
========================

Application Notes:
     - Endfire 66' / 167 cm Distance between front Screens cardiod Configuration 
     - Time aligned when front Subwoofer Screen and Top are in the same Distance
     - Linear Phase Latency included
     - Low passed at 100 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - Front: Ch. 1 
     - Module out 2 -  Back: Ch. 2 (Use front connector) 

Technical Info:
     - Fingerprint version: V1.0

=======================
Designed by ADAMSON & DV2
