Lab.Gruppen (P)LM Series module preset suitable for TW AUDiO VERA10-BIAMP and L24 speaker

Preset version: 3.10

Application notes:
* biamp: VERA10 biamp-flat, three boxes connected in parallel together with one L24 
* ATTENTION! Three physical outputs are needed. Patch L24 on 2+/- of the second output. 
* The Gain of L24 is adjustable. 
* Module contains three additional overlays with preconfigured filters: 
* 1. array size correction - changing filter gain according to VERTICAL ARRAY CORRECTION section from preset guide
* 2. 120 degrees - un-bypass overlay for entire array equipped with 120 degrees horn version 
* 3. LF extension - for adjustment of V10 together with L24.

Technical info:
* Amp Gain is 32 dB
* Set MaxPeak Level to 3 dB for usage with PLM(+) Series
* Set MaxPeak Level to 0 dB for usage with LM44 or LM26

Support information:
* E-Mail:   support@twaudio.com
* Internet: https://twaudio.de/en/
* Phone:    +49 (0) 71 41 - 48 89 89 55

Compilation date: 04/12/2024