Lake series preset suitable for TOA HX series speakers

Application Notes:
* Amp Gain is 35 dB
No ISVPL setting configured

HX-7 is 2 way speaker system that can change the vertical directivity 
angle and constant directivity control over a wide band that adopts 
the same phase wavefront control technology with FB-150 subwoofer 

HX-7   250W@8ohms
FB-150 200W@8ohms