Lab.gruppen's PLM Series preset suitable for JBL's VTX V25-II speaker, Rel 2.1

Application notes:
The preset is designed for fill application, high-passed at 60 Hz.
The filter is FIR and output 3 is HF, output 2 MF and output 1 LF.
Totallatency is 6.35 ms to match system performance.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +8 dBu (LF), 6.5 dBu (MF)5 and 2.5 dBu (HF)
* ISVPL thresholdat 177 Vpk (LF), 170 Vpk (MF) and 183 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
 
