Lab.gruppen's PLM Series preset suitable for JBL's VRX932LA speaker.

Application info:
VRX932LA multiple cabinets, active 2-way module.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), -2 dBu (HF)
* ISVPL threshold at 109.6 Vpk (LF), 43.6 (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11 dBu-pk (LF), +3 dBu-pk (HF)
* To emulate 26 dB Amp Gain - set input gain to -6 dB

Fingerprint: VRX932LA Bi-amplified v1.0b1 BETA