Lake preset for ADAMSON E219
========================

Application Notes:
     - Omni-directional module with 3 outputs for different output level / delay
     - No linear phase compensation delay included (add 5 ms for linear phase compensation)
     - Low passed at 100 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - E219 1
     - Module out 2 - E219 2 
     - Module out 3 - E219 3
 
Technical Info:
     - Fingerprint: V1.0

=======================
Designed by ADAMSON & DV2