Outline's PLM Series presets suitable for Outline's High Pack CDH483 & Low pack CDL1815

Application notes:
4-way module for High Pack CDH483 + Low Pack CDL1815.

Amp.Gain 35 dB

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +5 dBu (LOW PACK 18"), +2dbu (LOW PACK 15"), +3 dBu (HIGH PACK MF), -2 dBu (HIGH PACK HF)
* ISVPL threshold at 153.0 Vpk (LOW PACK 18"), 109.0 Vpk (LOW PACK 15"), 123.0 Vpk (HIGH PACK MF), 69.2 Vpk (HIGH PACK HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a Max-Peak limiter threshold at 
   
  +11 dBu-pk (LOW PACK 18"), +8 dBu-pk (LOW PACK 15"), +9 dBu-pk (MF), +4 dBu-pk (HF)