Lab.gruppen's PLM Series preset suitable for L-Acoustics' 115FM speaker.

Application notes:
The preset is designed for a monitor application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +7 dBu (LF), +4 dBu (HF)
* ISVPL threshold at 97.7 Vpk (LF), 69.2 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +10 dBu-pk (LF), +7 dBu-pk (HF)

Fingerprint info:
115FM v1.0 beta1