Lab.gruppen's PLM Series preset suitable for L-Acoustics' KIVA speaker with SB15 sub. v5.8

Application notes:
The module file is a 2-way configuration, high-passed at 100 Hz.
The Kiva filter is FIR and only output 3 is possible. SB15 is on output 1
Delay range is 0 - 20ms for both enclosures for flexible placement

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +3 dBu (Kiva), +9 dBu (SB15)
* ISVPL threshold at 142 Vpk (Kiva), 143 Vpk (SB15)
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +14 dBu-pk (Kiva), +16 dBu-pk (SB15)

