Adamson's PLM Series preset for Adamson's SpekTrix speaker.

Application Notes:
     The preset is high-passed at 60 Hz 24dB Linkwitz Riley.
     Maximum of 4 drivers in parallel per amplifier.
     Spek-Trix 5W mode to be used with Infra Sub.

Routing:
     SPB : 1
     LF : 2
     MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME