Lab.gruppen's PLM Series preset suitable for L-Acoustics' 12XT speaker.

Application notes:
The preset is designed for a fill application, high-passed at 100 Hz,
using the speaker in active mode.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +6 dBu (LF), +3 dBu (HF)
* ISVPL threshold at 109.5 Vpk (LF), 77.6 (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11 dBu-pk (LF), +8 dBu-pk (HF)