*** TURBOSOUND TQ Series                                    ***
*** V1.2 XP RELEASE                                         ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02 ***
*** All MODULES ARE CONTOUR XP FORMAT                       ***
***         README                                          ***

____________________________________________________
CHANGES: 

* Time alignment & polarity reversed for Subwoofer MODELS
** ISVLP OPTIMISATION UPDATE ALL MODELS
____________________________________________________

        HARDWARE LOCKING

ALL TURBOSOUND TQ SERIES LOUDSPEAKERS EXCLUSIVLY USE LAKE PRE-SETS VIA LAB.GRUPPEN PLM+ AND D SERIES L PLATFORMS. 
NO OTHER AMPLIFIER AND DSP PLATFORMS ARE SUPPORTED.

LM SERIES PROCESSORS ARE NOT COMPATIBLE WITH THESE MODULES.
TURBOSOUND TQ SERIES MODULES WILL NOT LOAD INTO LM SERIES PROCESSORS.
____________________________________________________
MODULE OUTPUT MIXING IS NOT REQUIRED FOR 1.2 XP RELEASE
V1.1 MANCHESTER MODULES ARE NOT DESIGNED TO BE USED TOGETHER IN THE SAME SYSTEM WITH TQ - PLEASE USE MANCHESTER REV2.3 XP

PLEASE CONSULT THE QUICK START GUIDE FOR DETAILED INSTRUCTIONS
____________________________________________________

All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02

*** Designed by TURBOSUND - MAR 2024 ***
http://www.turbosound.com

