Lake series preset suitable for TOA HX series speakers

Application Notes:
* Amp Gain is 35 dB
ISVPL Setting 57.0V 

HX-5 that 2-way speaker system capable of constant directivity 
control over a wide band and change of vertical directivity 
angle with FB-120B subwoofer 

HX-5   200W@8ohms 
FB-120 200W@8ohms
