Lab.gruppen's PLM Series FIR preset suitable for Alcons LR16.

Application notes:
* Bi-amp 2-way configuration.
* LF on channel 1
* HF on channel 2
* Use respective Fly 3, 6, 9 or 12 Preset for whole array depending on number of boxes used
* Mid range array size compensation EQ used for size of array

Technical info:
* Amp Gain is 32 dB
* ISVPL threshold at 89.7 Vpk(LF) and 32.6 Vpk(HF)
* Delay set on 80Hz and 160Hz presets to align with LR16B presets, FR presets have no delay